User application Displays or logs data

Register Device Driver with I2C Subsystem

Initialize I2C Adapter in BBB

Return Data to user application

Initialize MPU-6050

Create Device Node (eg., /dev/accel0)

Wait for read request from user space